{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["配置清单"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"配置清单","index":0,"n_rows":15,"n_cols":9,"rows_kept":15,"merged":[[0,0,0,7],[2,0,2,7],[14,1,14,5],[14,6,14,7]],"flags":["formulas_cached_only"]}
["配置清单"]
["项目","产品名称/规格","型号","单位","数量","单价","小计","备注"]
["门禁系统"]
[1,"网络型主控模块","NAC-9000N-KIT","台 ",9,null,0,"网络型主控模块，支持TCP/IP、CAN、RS485通讯方式，配合NAC9004B、NAC9002B使用。含机箱、16.5V/3A变压器、12V/3.2AH蓄电池。"]
[2,"两门门禁控制模块","NAC9002B-KIT","台 ",113,null,0,"两门门禁控制模块，支持CAN通讯方式。含机箱、16.5V/3A变压器、12V/3.2AH蓄电池。"]
[3,"IC卡读卡器","NR-3A-WBN","块",226,null,0,"Type A(Mifare 1)读卡器、NITRO品牌、韦根34位（32位，26位）输出（可选）、86-I款外形、黑色（灰色，蓝色，白色可选，订货注明）外壳"]
[4,"电插锁","NDL-250","只",18,null,0,"埋入式阳极锁, 5线,断电开型时间可调,按钮输入与监督输出","用于双开玻璃门"]
[5,"阳极锁外挂架","NR-100","只",18,null,0,"阳极锁外挂架,适用外挂安装在90°或180°开之各式门"]
[6,"阳极锁不锈钢玻璃夹","NG-110","只",18,null,0,"阳极锁不锈钢玻璃夹,适于无框玻璃门须与NR-100搭配"]
[7,"磁力锁","NML-G6B","只",123,null,0,"外挂式埋入型600磅拉力磁力锁,具双色指示灯与监督输出","用于消防门"]
[8,"磁力锁辅助支架","NE-G6B","只",123,null,0,"磁力锁辅助支架,与600磅磁力锁使用,适用于内推门"]
[9,"IC卡发卡器","NR-3A-UNH","个",1,null,0,"IC卡发卡器，Mini外形、NITRO品牌、USB接口输出、模拟电脑键盘接口，只读IC卡CSN、USB接口、浅蓝色外壳。支持SecNET桌面发卡。"]
[10,"网络门禁控制软件完整版","SecNET-9000N","套",1,null,0,"门禁控制软件完整版，持卡人数量无限制，控制器台数无限制，具有电子地图，考勤功能，支持NAC-9000N系列门禁控制器。"]
[11,"管理电脑","自配","台",1,null,0,"I5以上，4G内存"]
[12,"合计",{"$nulls":4},0]